[E129]\_[E130] Boil and mash lids

This document is suitable for changing both of the lids. Lids are kept in place by the indicated screws and nuts.



Unscrew the screws and remove the lid.




Replace the lid.

After reassembling, lids must be positioned.






You can also adjust by the lid fixing holes.











You can also adjust by the lid fixing holes.

