[E146] Polishing instructions

In some cases, the bottom of the tanks can burn down so that the burned material cannot be removed only by washing. To remove the burned residues, you can use a wet (pour 1 dL water into the affected tank), fine grit (K600) sandpaper to sand the metal surface.

**IMPORTANT:** sand the surface using sharp, unidirectional movements (in the direction of the grooves) to avoid unnecessary scratches.

**IMPORTANT:** plug the tank before sanding to avoid falling metal swarf in the piping system as it may damage it.

**IMPORTANT:** clean the machine properly after sanding.