

[E119] Front panel



Unscrew the front panel fixing screws.







Push down the front panel to pop it out.



Disconnect the indicated plugs from the front panel (button cables, USB and the red No.04 cable).




Replace the front panel unit.



Put the original SD card to the new Front panel!





Reassemble consists of the same steps in reverse.